**Ambush Ice House Talking Points**

The Ambush skid houses are built to last and take abuse

* **Aluminum frame construction**
  + Strong and lightweight
    - Stryker - 620 pounds
    - Slayer - 1,050 pounds (estimate)
* **No Wood**
  + There is no wood in the entire ice house, including the floor, that can rot or delaminate.
    - Snow from boots or slush from drilling holes will not deteriorate the floor
* **Strong, one piece chassis and skiis**
  + Hitch attachment points run the length of the chassis
  + Break loose from ice without damage to ice house
  + Rugged across rough ice and snow
  + Long lasting
  + Tow from either direction
* **Floor**
  + 2-¼” thick
  + Multiple layers
  + Insulated
  + NO wood
  + Catch covers pre installed ready to fish
  + Add more catch covers in between studs in floor
* **No Seams**
  + Seams in sidewalls or roofs can cause water penetration and eventually work loose.
  + Nice clean look
* **Gelcoat exterior**
  + Nice look
  + Easy to clean
  + Durable (same material as many boat hulls)
* **Finished interior**
  + Ready to fish
  + Pleasant and comfortable fishing environment
* **Clean Grip floor**
  + Slip resistant
  + Rugged
  + Non wood
* **Ambush durabond panel system™:**
  + The walls, roof and floor are constructed with layers of materials laminated together which form a “sandwich” with insulated styrofoam in the middle providing comfort and warmth
  + The lamination process increases strength
  + No mechanical fasteners in the process that can work loose
* Weight
  + Stryker - 620#
  + Slayer - 880#
* Height
  + Stryker & Slayer
    - Outside peak - 92”
    - Inside peak - 81”
* A 200 pound person is about 2.08 pounds per square inch on the ice
* Stryker with nobody in it is .625 pounds per square inch
* Stryker with (2) 200 pound males is 1.02 pounds per square inch
* R values:
  + Floor - 12
  + Roof - 7
  + Walls - 5