**Ambush Ice House Talking Points**

The Ambush skid houses are built to last and take abuse

* **Aluminum frame construction**
	+ Strong and lightweight
		- Stryker - 620 pounds
		- Slayer - 1,050 pounds (estimate)
* **No Wood**
	+ There is no wood in the entire ice house, including the floor, that can rot or delaminate.
		- Snow from boots or slush from drilling holes will not deteriorate the floor
* **Strong, one piece chassis and skiis**
	+ Hitch attachment points run the length of the chassis
	+ Break loose from ice without damage to ice house
	+ Rugged across rough ice and snow
	+ Long lasting
	+ Tow from either direction
* **Floor**
	+ 2-¼” thick
	+ Multiple layers
	+ Insulated
	+ NO wood
	+ Catch covers pre installed ready to fish
	+ Add more catch covers in between studs in floor
* **No Seams**
	+ Seams in sidewalls or roofs can cause water penetration and eventually work loose.
	+ Nice clean look
* **Gelcoat exterior**
	+ Nice look
	+ Easy to clean
	+ Durable (same material as many boat hulls)
* **Finished interior**
	+ Ready to fish
	+ Pleasant and comfortable fishing environment
* **Clean Grip floor**
	+ Slip resistant
	+ Rugged
	+ Non wood
* **Ambush durabond panel system™:**
	+ The walls, roof and floor are constructed with layers of materials laminated together which form a “sandwich” with insulated styrofoam in the middle providing comfort and warmth
	+ The lamination process increases strength
	+ No mechanical fasteners in the process that can work loose
* Weight
	+ Stryker - 620#
	+ Slayer - 880#
* Height
	+ Stryker & Slayer
		- Outside peak - 92”
		- Inside peak - 81”
* A 200 pound person is about 2.08 pounds per square inch on the ice
* Stryker with nobody in it is .625 pounds per square inch
* Stryker with (2) 200 pound males is 1.02 pounds per square inch
* R values:
	+ Floor - 12
	+ Roof - 7
	+ Walls - 5